To find the delay given by the filter, I remembered the path consisted of half a ‘wavelength’ like I did in the angle calculations. So to figure out the time that each electron spent in the filter, I took have a period and added the time calculated before for the small deflection at the end of the path.

Combining this equation with the angle one, gives the following equation.

Below is that graph against the program’s data.



